Text 3

|  |
| --- |
| DESCALING INSTRUCTIONS* IN HARD WATER AREAS REGULAR DESCALING IS ESSENTIAL TO KEEP YOUR KETTLE IN GOOD WORKING ORDER.
* If your kettle switches off before it has boiled it indicates your kettle needs descaling.
* Descale your kettle using
	+ either a proprietary kettle descaler suitable for PLASTIC kettles. Follow manufacturer's instructions,
	+ or white vinegar
		1. Fill the kettle with ½ l of 8° white vinegar.
		2. Leave to soak for 1 hour without boiling.
		3. Empty your kettle and rinse it two or three times with clear water.
	+ or citric acid
		1. Boil 0.5 l of water.
		2. Add 25 g of citric acid.
		3. Leave to soak for 15 minutes.
		4. Discard this mixture.
		5. Rinse the kettle with clear water two or three times.
* Repeat process if needed.
* Descaling agents for metal kettles, coffee makers or steam irons are unsuitable and will damage your Tefal kettle. Never use metal abrasives to clean the interior.
* When using powder descaler or citric acid, always add water. Never use in an empty kettle.
* Always follow the directions for use on the descaler carefully. Rinse the inside well after using a descaler.
 |