Text 3

|  |
| --- |
| DESCALING INSTRUCTIONS   * IN HARD WATER AREAS REGULAR DESCALING IS ESSENTIAL TO KEEP YOUR KETTLE IN GOOD WORKING ORDER. * If your kettle switches off before it has boiled it indicates your kettle needs descaling. * Descale your kettle using   + either a proprietary kettle descaler suitable for PLASTIC kettles. Follow manufacturer's instructions,   + or white vinegar     1. Fill the kettle with ½ l of 8° white vinegar.     2. Leave to soak for 1 hour without boiling.     3. Empty your kettle and rinse it two or three times with clear water.   + or citric acid     1. Boil 0.5 l of water.     2. Add 25 g of citric acid.     3. Leave to soak for 15 minutes.     4. Discard this mixture.     5. Rinse the kettle with clear water two or three times. * Repeat process if needed. * Descaling agents for metal kettles, coffee makers or steam irons are unsuitable and will damage your Tefal kettle. Never use metal abrasives to clean the interior. * When using powder descaler or citric acid, always add water. Never use in an empty kettle. * Always follow the directions for use on the descaler carefully. Rinse the inside well after using a descaler. |